vers(a, {-$OpenBSD: MAKEDEV.common,v 1.75 2014/07/15 17:36:13 miod Exp $-})dnl
dnl
dnl Copyright (c) 2001-2006 Todd T. Fries <todd@OpenBSD.org>
dnl
dnl Permission to use, copy, modify, and distribute this software for any
dnl purpose with or without fee is hereby granted, provided that the above
dnl copyright notice and this permission notice appear in all copies.
dnl
dnl THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
dnl WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
dnl MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
dnl ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
dnl WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
dnl ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF
dnl OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
dnl
dnl Common device definitions.
dnl
dnl This file contains the MI device definitions (as well as some MD
dnl definitions not cleaned up yet...)
dnl
dnl Diversions:  (upon termination, concatenated output queues)
dnl
dnl 0 - very top
dnl 1 - descriptions of devices
dnl 2 - init of script, function definitions, etc
dnl 3 - beginning of global recursive R() function
dnl 7 - body of MAKEDEV, device creations, etc
dnl 9 - end
dnl
dnl Diversions 2, 3 and 7 are not filled when generating the manual page.
dnl
dnl HOW TO ADD A DEVICE:
dnl
dnl In this file, you must use at least two macros:
dnl
dnl  Use '__devitem(uniqueid, name-pattern, description)' to create an entry
dnl  in the description at the top of the generated MAKEDEV file:
dnl
dnl    __devitem(sca, sca*, Sugar Generic device)dnl
dnl    __devitem(cry, crypto, hardware crypto access driver)dnl
dnl
dnl  This is ultimately shown as:
dnl
dnl    #  sca*   Sugar Generic device
dnl    #  crypto hardware crypto access driver
dnl
dnl  Use '_mkdev(uniqueid, shell-pattern, {-shell-script-})dnl' to create
dnl  a shell script fragment used to 'create' the device (be sure to match
dnl  the uniqueid from above):
dnl
dnl    _mkdev(sca, sca*, {-M sca$U c major_sca_c $U
dnl           M rsca$U b major_sca_b Add($U, 128)-})dnl
dnl    _mkdev(cry, crypto, {-M crypto c major_cry_c 0-})dnl
dnl
dnl  This is ultimately expanded into:
dnl
dnl    sca*)
dnl           M sca$U c 24 $U
dnl           M sca$U b 42 $(($U+128))
dnl           ;;
dnl
dnl    crypto)
dnl           M crypto c 47 0
dnl           ;;
dnl
dnl In the MAKEDEV.md file, add a '_DEV(uniqueid, charmajor, blockmajor)'
dnl entry:
dnl
dnl   _DEV(sca, 24, 42)
dnl   _DEV(cry, 47)
dnl
dnl Final step is to use the 'target/twrget' macros to have the 'all)' target
dnl generate one or more device(s).  Usage of 'target/twrget' is:
dnl      target(target_name, device_name [, append_string ] .. )
dnl      twrget(target_name, uniqueid, device_name, [, append_string ] .. )
dnl
dnl        target_name   a unique name that later is used as an argument to
dnl                      'show_target()' (which expands all devices for a
dnl                      given 'target_name').
dnl        uniqueid      same as 'uniqueid' above
dnl        device_name   string representing the device to be mknod'ed
dnl        append_string for each append_string, `device_name' is prepended
dnl
dnl Note: 'target(a,b,c)' is equivalent to 'twrget(a,b,b,c)'
dnl
dnl
dnl For a short example:
dnl
dnl   target(all, std)dnl
dnl   target(all, sca, 0, 1, 2, 3)dnl
dnl   twrget(all, cry, crypto)dnl
dnl
dnl would expand to:
dnl
dnl   all)
dnl        R std sca0 sca1 sca2 sca3 crypto
dnl        ;;
dnl
dnl presuming '_DEV(sca, ?, ?)' and '_DEV(std)' were in the MAKEDEV.md file.
dnl
dnl
dnl Everything is 'automatically' added to 'MAKEDEV' based on whether or
dnl not the '_DEV()' entry has a corresponding _mkdev() and __devitem()
dnl entry in MAKEDEV.mi (this file).
dnl
dnl Note: be very wary of adding whitespace, carriage returns, or not
dnl finishing a macro with ')dnl' .. otherwise, extra blank lines show up
dnl in the output.
dnl
dnl TODO:
dnl
dnl make a 'disktgt' macro that automatically does:
dnl disktgt(rd, {-rd-})
dnl
dnl	target(all,rd,0)
dnl	target(ramd,rd,0)
dnl	disk_q(rd)
dnl	__devitem(rd, {-rd*-}, {-rd-})dnl
dnl
dnl  Note: not all devices are generated in 'all)' below. MAKEDEV.md contains
dnl        its own extra list.
dnl
divert(1)dnl
twrget(all, fdesc, fd)dnl
target(all, st, 0, 1)dnl
target(all, std)dnl
target(all, ra, 0, 1, 2, 3)dnl
target(all, rx, 0, 1)dnl
target(all, wd, 0, 1, 2, 3)dnl
target(all, xd, 0, 1, 2, 3)dnl
target(all, systrace)dnl
target(all, pctr)dnl
target(all, pctr0)dnl
target(all, pf)dnl
twrget(all, cry, crypto)dnl
target(all, apm)dnl
target(all, acpi)dnl
twrget(all, tth, ttyh, 0, 1)dnl
target(all, ttyA, 0, 1)dnl
target(all, ttyB, 0, 1, 2, 3, 4, 5)dnl
twrget(all, attyB, ttyB, 0, 1, 2, 3, 4)dnl
twrget(all, mac_tty0, tty0, 0, 1)dnl
twrget(all, tzs, tty, a, b, c, d)dnl
twrget(all, czs, cua, a, b, c, d)dnl
target(all, ttyc, 0, 1, 2, 3, 4, 5, 6, 7)dnl
twrget(all, com, tty0, 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, a, b)dnl
target(all, lkm)dnl
twrget(all, mmcl, mmclock)dnl
target(all, lpt, 0, 1, 2)dnl
twrget(all, lpt, lpa, 0, 1, 2)dnl
target(all, joy, 0, 1)dnl
twrget(all, rnd, random)dnl
target(all, uk, 0)dnl
twrget(all, vi, video, 0, 1)dnl
twrget(all, speak, speaker)dnl
target(all, asc, 0)dnl
target(all, radio, 0)dnl
target(all, tuner, 0)dnl
target(all, rmidi, 0, 1, 2, 3, 4, 5, 6, 7)dnl
target(all, uall)dnl
target(all, pci, 0, 1, 2, 3)dnl
twrget(all, wsmouse, wscons)dnl
target(all, par, 0)dnl
target(all, apci, 0)dnl
target(all, local)dnl
target(all, gpr, 0)dnl
target(all, ptm)dnl
target(all, hotplug)dnl
target(all, pppx)dnl
target(all, fuse)dnl
dnl
_mkdev(all, {-all-}, {-dnl
show_target(all)dnl
-})dnl
dnl
dnl XXX some arches use ramd, others ramdisk - needs to be fixed eventually
__devitem(ramdisk, ramdisk, Ramdisk kernel devices,nothing)dnl
dnl
target(usb, usb, 0, 1, 2, 3, 4, 5, 6, 7)dnl
target(usb, urio, 0)dnl
target(usb, uhid, 0, 1, 2, 3)dnl
target(usb, ulpt, 0, 1)dnl
target(usb, ugen, 0, 1, 2, 3, 4, 5, 6, 7)dnl
target(usb, ttyU, 0, 1, 2, 3)dnl
dnl
__devitem({-uall-}, uall, All USB devices,usb)dnl
_mkdev(uall, uall, {-dnl
show_target({-usb-})dnl
-})dnl
__devtitle(tap, Tapes)dnl
__devitem(tz, tz*, {-DEC TK50 cartridge tape drives-})dnl
__devitem(st, {-st*-}, SCSI tape drives)dnl
_mkdev(st, st*, {-n=Mult($U, 16)
	for pre in " " n e en
	do
		M ${pre}st$U	b major_st_b $n 660 operator
		M ${pre}rst$U	c major_st_c $n 660 operator
		n=Add($n, 1)
	done-})dnl
__devitem(mt, mt*, (Magnetic) 9-track reel tape drives)dnl
__devtitle(dis, Disks)dnl
__devitem(sd, {-sd*-}, {-SCSI disks{-,-} including flopticals-})dnl
__devitem(cd, {-cd*-}, ATAPI and SCSI CD-ROM drives)dnl
_mkdev(cd, cd*, {-dodisk2 cd $U major_cd_b major_cd_c $U 0{--}ifstep(cd)-})dnl
__devitem(fuse, fuse, Userland Filesystem, fuse 4)dnl
_mcdev(fuse, fuse, fuse, {-major_fuse_c-}, 600)dnl
__devitem(ch, {-ch*-}, SCSI media changers)dnl
_mcdev(ch, ch*, ch, {-major_ch_c-}, 660, operator)dnl
__devitem(uk, uk*, Unknown SCSI devices)dnl
_mcdev(uk, uk*, uk, {-major_uk_c-}, 640, operator)dnl
dnl XXX see ramdisk above
__devitem(ramd, ramdisk, Ramdisk kernel devices,nothing)dnl
dnl
_mkdev(ramd, ramdisk, {-dnl
show_target(ramd)dnl
-})dnl
dnl
target(ramd, std)dnl
target(ramd, bpf, 0)dnl
twrget(ramd, com, tty0, 0, 1)dnl
target(ramd, sd, 0, 1, 2, 3, 4)dnl
target(ramd, wd, 0, 1, 2, 3, 4)dnl
target(ramd, st, 0, 1)dnl
target(ramd, cd, 0, 1)dnl
target(ramd, rd, 0)dnl
dnl
__devitem(rd, {-rd*-}, quote(rd)pseudo-disks)dnl
_mkdev(rd, rd*, {-dodisk2 rd $U major_rd_b major_rd_c $U 0{--}ifstep(rd)-})dnl
__devitem(xd, xd*, Xylogic 753/7053 disks)dnl
__devitem(xy, xy*, {-	Xylogic 450/451 disks-})dnl
__devitem(flo, {-fd*-}, {-Floppy disk drives (3 1/2"{-,-} 5 1/4")-},fd)dnl
_mkdev(flo, fd*,
{-typnam=$U${i#fd[01]*}
	case $typnam in
	0|1)	typnum=0;; # no type specified, assume A
	*A)	typnum=0; typnam=0;;
	*B)	typnum=1;;
	*C)	typnum=2;;
	*D)	typnum=3;;
	*E)	typnum=4;;
	*F)	typnum=5;;
	*G)	typnum=6;;
	*H)	typnum=7;;
	*)	echo bad type $typnam for $i; exit 1;;
	esac
	case $U in
	0|1)	blk=major_flo_b; chr=major_flo_c;;
	*)	echo bad unit $U for $i; exit 1;;
	esac
	nam=fd${typnam}
	n=Add(Mult($U, 128), Mult($typnum, 16))
	M ${nam}a	b $blk $n 640 operator
	M ${nam}b	b $blk Add($n, 1) 640 operator
	M ${nam}c	b $blk Add($n, 2) 640 operator
	M ${nam}i	b $blk Add($n, 8) 640 operator
	M r${nam}a	c $chr $n 640 operator
	M r${nam}b	c $chr Add($n, 1) 640 operator
	M r${nam}c	c $chr Add($n, 2) 640 operator
	M r${nam}i	c $chr Add($n, 8) 640 operator-}, 664)dnl
__devitem(wd, {-wd*-}, {-quote(winchester)disk drives (ST506{-,-} IDE{-,-} ESDI{-,-} RLL{-,-} ...)-})dnl
__devitem(vnd, vnd*, quote(file)pseudo-disk devices)dnl
_mkdev(vnd, vnd*, {-dodisk vnd $U major_vnd_b major_vnd_c $U 0{--}ifstep(vnd)-})dnl
__devitem(ra, ra*, {-MSCP disks-})dnl
__devitem(rx, rx*, {-RX02 floppy disks-})dnl
dnl
dnl For normal disk devices, add a disk_q entry; anything else define like
dnl the rest (such as vnd above).
dnl
disk_q({-hd-})dnl
disk_q({-ra-})dnl
disk_q({-rx-})dnl
disk_q({-sd-})dnl
disk_q({-xy-})dnl
disk_q({-xd-})dnl
disk_q({-wd-})dnl
_mkdev({-disks-}, {-undefine({-C_ase-})show_disks()undefine({-C_ase-})-},
{-case $i in
show_disks2()dnl
	esac-})dnl
__mkdev({-disks-}){--}dnl
dnl
__devtitle(cons, Console ports)dnl
__devitem(wscons, wscons, Minimal wscons devices)dnl
twrget(wscons, wscons, ttyC, cfg, 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, a, b)dnl
target(wscons, wsmux)dnl
target(wscons, wskbd, 0, 1, 2, 3)dnl
target(wscons, wsmouse, 0, 1, 2, 3)dnl
_mkdev({-wscons-}, {-wscons-}, {-dnl
show_target(wscons)dnl
-})dnl
__devitem(wsdisp, ttyC-J*, wscons display devices,wsdisplay)dnl
_mkdev({-wsdisp-}, tty[C-J]*, {-U=${i##tty[C-J]}
	case $i in
	ttyC*) n=C m=expr(0*256);;
	ttyD*) n=D m=expr(1*256);;
	ttyE*) n=E m=expr(2*256);;
	ttyF*) n=F m=expr(3*256);;
	ttyG*) n=G m=expr(4*256);;
	ttyH*) n=H m=expr(5*256);;
	ttyI*) n=I m=expr(6*256);;
	ttyJ*) n=J m=expr(7*256);;
	esac
	case $U in
	[0-9a-f]) M tty$n$U c major_wsdisp_c Add(16#$U, $m) 600;;
	cfg) M tty${n}cfg c major_wsdisp_c Add(255,$m) 600;;
	*) echo bad unit $U for $i; exit 1;;
	esac-})dnl
__devitem(wskbd, wskbd*, wscons keyboards)dnl
dnl XXX wskbd[0-9]* instead of wskbd* in case this appears before
dnl XXX ``wsmux|wsmouse|wskbd'' in the final MAKEDEV.
_mkdev(wskbd, wskbd[0-9]*, {-M wskbd$U c major_wskbd_c $U 600-})dnl
__devitem(wsmux, wsmux, wscons keyboard/mouse mux devices)dnl
_mkdev(wsmux, wsmux|wsmouse|wskbd, {-M wsmouse c major_wsmux_c 0 600
	M wskbd c major_wsmux_c 1 600-})dnl
__devitem(pcons, console, PROM console)dnl
__devtitle(point, Pointing devices)dnl
__devitem(wsmouse, wsmouse*, wscons mice)dnl
dnl XXX wsmouse[0-9]* instead of wsmouse* in case this appears before
dnl XXX ``wsmux|wsmouse|wskbd'' in the final MAKEDEV.
_mkdev(wsmouse, wsmouse[0-9]*, {-M wsmouse$U c major_wsmouse_c $U 600-})dnl
__devtitle(pty, Pseudo terminals)dnl
__devitem(ptm, ptm, pty master device)dnl
_mkdev(ptm, ptm, {-M ptm c major_ptm_c 0 666-})dnl
__devitem(tty, tty*, Set of 62 slave pseudo terminals)dnl
__devitem(pty, pty*, Set of 62 master pseudo terminals)dnl
_mkdev(pty, pty*, {-if [ $U -gt 15 ]; then
		echo bad unit for pty in: $i
		continue
	fi
	set -A letters p q r s t u v w x y z P Q R S T
	set -A suffixes 0 1 2 3 4 5 6 7 8 9 a b c d e f g h i j k l m n o p q \
	    r s t u v w x y z A B C D E F G H I J K L M N O P Q R S T U V W X \
	    Y Z

	name=${letters[$U]}
	n=0
	while [ $n -lt 62 ]
	do
		nam=$name${suffixes[$n]}
		off=Mult($U, 62)
		M tty$nam c major_tty_c Add($off, $n)
		M pty$nam c major_pty_c Add($off, $n)
		n=Add($n, 1)
	done-})dnl
__devitem(dc, dc*, {-4 channel serial interface (keyboard{-,-} mouse{-,-}modem{-,-} printer)-})dnl
__devitem(drm, drm*, {-Direct Rendering Manager-})dnl
_mcdev({-drm-}, drm*, {-drm-}, {-major_drm_c-}, 600)dnl
__devtitle(prn, Printers)dnl
__devitem(lpt, lpt*, IEEE 1284 centronics printer)dnl
_mkdev(lpt, lpt*|lpa*,
{-case $i in
	lpt*) n=lpt f=0;;
	lpa*) n=lpa f=128;;
	esac
	M $n$U c major_lpt_c Add($U, $f) 600-})dnl
__devitem(lpa, lpa*, Polled printer port,lpt)dnl
__devtitle({-usb-}, USB devices)dnl
__devitem({-usb-}, usb*, Bus control devices used by usbd for attach/detach)dnl
_mkdev({-usb-}, usb*, {-[ "$i" = "usb" ] && u= || u=$U
	M usb$u c major_usb_c $U 660-})dnl
__devitem(uhid, uhid*, Generic HID devices)dnl
_mcdev({-uhid-}, uhid*, {-uhid-}, {-major_uhid_c-}, 660)dnl
__devitem(ulpt, ulpt*, Printer devices)dnl
_mcdev({-ulpt-}, ulpt*, {-ulpt-}, {-major_ulpt_c-}, 660)dnl
__devitem(ttyU, ttyU*, USB serial ports,ucom)dnl
_mkdev({-ttyU-}, {-ttyU[0-9a-zA-Z]-}, {-U=${i#ttyU*}
	o=$(alph2d $U)
	M ttyU$U c major_ttyU_c $o 660 dialer uucp
	M cuaU$U c major_ttyU_c Add($o, 128) 660 dialer uucp-})dnl
__devitem(urio, urio*, Diamond Multimedia Rio 500)dnl
_mcdev({-urio-}, urio*, {-urio-}, {-major_urio_c-}, 660)dnl
__devitem(ugen, ugen*, Generic USB devices)dnl
_mkdev(ugen, ugen*, {-n=Mult($U, 16)
	for j in 0{0,1,2,3,4,5,6,7,8,9} 1{0,1,2,3,4,5}
	do
		M ugen$U.$j c major_ugen_c Add($n, 10#$j) 660
	done-})dnl
__devtitle(call, Call units)dnl
__devtitle(term, Terminal ports)dnl
__devitem(dca, dca*, HP200/300 single port serial interface)dnl
__devitem(dcm, dcm*, HP200/300 4 port serial mux interface)dnl
__devitem(apci, apci*, HP400 4 port serial mux interface)dnl
__devitem({-com-}, {-tty[0-7][0-9a-f]-}, NS16x50 serial ports)dnl
_mkdev(com, {-tty[0-7][0-9a-f]-}, {-U=${i#tty*}
	o=$(h2d $U)
	M tty$U c major_com_c $o 660 dialer uucp
	M cua$U c major_com_c Add($o, 128) 660 dialer uucp-})dnl
__devitem(ttyc, ttyc*, Cyclades serial ports,cy)dnl
__devitem(tzs, tty[a-z]*, Zilog 8530 Serial Port,zs)dnl
_mkdev(tzs, {-tty[a-z]-}, {-u=${i#tty*}
	case $u in
	a) n=0 ;;
	b) n=1 ;;
	c) n=4 ;;
	d) n=5 ;;
	*) echo unknown tty device $i ;;
	esac
	M tty$u c major_tzs_c $n 660 dialer uucp-})dnl
__devitem(tth, ttyh*, Sab82532 serial devices,sab)dnl
_mkdev(tth, ttyh*, {-M ttyh$U c major_tth_c $U 660 dialer uucp-})dnl
__devitem(czs, cua[a-z]*, Zilog 8530 Serial Port,zs)dnl
_mkdev(czs, cua[a-z], {-u=${i#cua*}
	case $u in
	a) n=0 ;;
	b) n=1 ;;
	c) n=4 ;;
	d) n=5 ;;
	*) echo unknown cua device $i ;;
	esac
	M cua$u c major_czs_c Add($n, 128) 660 dialer uucp-})dnl
__devitem(tty0, tty00, Standard serial port,com)dnl
__devitem(mac_tty0, tty00, Standard serial port,zsc)dnl
__devitem(ttyz, tty[a-d], On-board zs serial ports,zs)dnl
__devitem(cuaz, cua[a-d], On-board zs serial ports,zs)dnl
__devitem(ttyB, ttyB?, DEC 3000 ZS8530 ("scc") serial ports,scc)dnl
__devitem(scc, scc*, 82530 serial interface,scc)dnl
__devtitle(spec, Special purpose devices)dnl
_mkdev(apm, apm*, {-M apm	c major_apm_c 0 644
	M apmctl	c major_apm_c 8 644-})dnl
_mkdev(acpi, acpi*, {-M acpi	c major_acpi_c 0 644-})dnl
__devitem(pctr, pctr*, PC Performance Tuning Register access device)dnl
_mkdev(pctr, pctr, {-M pctr c major_pctr_c 0 644-})dnl
__devitem(systrace, systrace*, System call tracing device)dnl
_mkdev(systrace, systrace, {-M systrace c major_systrace_c 0 644-})dnl
__devitem(au, audio*, Audio devices,audio)dnl
_mkdev(au, audio*, {-M sound$U	c major_au_c $U
	M mixer$U	c major_au_c Add($U, 16)
	M audio$U	c major_au_c Add($U, 128)
	M audioctl$U	c major_au_c Add($U, 192)
	MKlist[${#MKlist[*]}]=";[ -e audio ] || ln -s audio$U audio"
	MKlist[${#MKlist[*]}]=";[ -e mixer ] || ln -s mixer$U mixer"
	MKlist[${#MKlist[*]}]=";[ -e sound ] || ln -s sound$U sound"
	MKlist[${#MKlist[*]}]=";[ -e audioctl ] || ln -s audioctl$U audioctl"-})dnl
__devitem(vi, video*, Video V4L2 devices,video)dnl
_mkdev(vi, video*, {-M video$U  c major_vi_c $U
	MKlist[${#MKlist[*]}]=";[ -e video ] || ln -s video$U video"-})dnl
__devitem(asc, asc*, ASC Audio device)dnl
_mkdev(asc, asc*, {-M asc$U major_asc_c 0-})dnl
__devitem(bio, bio, {-ioctl tunnel pseudo-device-})dnl
_mkdev(bio, bio, {-M bio c major_bio_c 0 600-})dnl
__devitem(radio, radio*, FM tuner devices)dnl
_mkdev(radio, radio*, {-M radio$U     c major_radio_c $U
	MKlist[${#MKlist[*]}]=";[ -e radio ] || ln -s radio$U radio"-})dnl
__devitem(fdesc, fd, fd/* nodes, fd)dnl
_mkdev(fdesc, fd, {-RMlist[${#RMlist[*]}]=";mkdir -p fd;rm -f" n=0
	while [ $n -lt 64 ];do M fd/$n c major_fdesc_c $n;n=Add($n, 1);done
	MKlist[${#MKlist[*]}]=";chmod 555 fd"-})dnl
__devitem(oppr, openprom,PROM settings,openprom)dnl
_cdev(oppr, openprom, 70, 0)dnl
__devitem(cry, crypto, Hardware crypto access driver,crypto)dnl
_mkdev(cry, crypto, {-M crypto c major_cry_c-} 0)dnl
__devitem(pf, pf*, Packet Filter)dnl
_mkdev(pf, {-pf*-}, {-M pf c major_pf_c 0 600-})dnl
__devitem(bpf, bpf*, Berkeley Packet Filter)dnl
_mkdev(bpf, {-bpf*-}, {-M bpf$U c major_bpf_c $U 600-}, 600)dnl
_mkdev(tun, {-tun*-}, {-M tun$U c major_tun_c $U 600-}, 600)dnl
__devitem(speak, speaker, PC speaker,spkr)dnl
_mkdev(speak, speaker, {-M speaker c major_speak_c 0 600-})dnl
__devitem(lkm, lkm, Loadable kernel modules interface)dnl
_cdev(lkm, lkm, {-major_lkm_c-}, 0, 640, _lkm)dnl
__devitem(tun, tun*, Network tunnel driver)dnl
__devitem(rnd, *random, In-kernel random data source,random)dnl
_mkdev(rnd, *random, {-n=0
	for pre in " " s u a
	do
		M ${pre}random c major_rnd_c $n 644
		n=Add($n, 1)
	done-}, 644)dnl
__devitem(joy, joy*, Joystick driver)dnl
_mcdev(joy, joy*, joy, {-major_joy_c-}, 666)dnl
__devitem(mag, magma*, Magma multiport cards,magma)dnl
__devitem(bppmag, bppmag[mno], Magma parallel port,magma)dnl
__devitem(spif, spif*, quote(spif)multiport cards)dnl
__devitem(bppsp, bpp[jkl], quote(spif)parallel port,spif)dnl
_mkdev(mag, magma*, {-case $U in
	0)	offset=0  nam=m;;
	1)	offset=16 nam=n;;
	2)	offset=32 nam=o;;
	*)	echo "bad unit for $i: $U"; exit 127;;
	esac
	offset=Mult($U, 64)
	n=0
	while [ $n -lt 16 ]
	do
		name=${nam}`hex $n`
		M tty$name c major_mag_c Add($offset, $n) 660 dialer uucp
		n=Add($n, 1)
	done
	M bpp${nam}0 c major_bppmag_c Add($offset, 0) 600
	M bpp${nam}1 c major_bppmag_c Add($offset, 1) 600-})dnl
_mkdev(spif, spif*, {-case $U in
	0)	offset=0  nam=j;;
	1)	offset=16 nam=k;;
	2)	offset=32 nam=l;;
	*)	echo "bad unit for $i: $U"; exit 127;;
	esac
	offset=Mult($U, 64)
	n=0
	while [ $n -lt 8 ]
	do
		name=${nam}`hex $n`
		M tty$name c major_spif_c Add($offset, $n) 660 dialer uucp
		n=Add($n, 1)
	done
	M bpp${nam}0 c major_bppsp_c Add($offset, 0) 600-})dnl
__devitem(bpp, bpp*, Parallel port)dnl
_mkdev(bpp, {-bpp*-}, {-M bpp$U c major_bpp_c $U 600-}, 600)dnl
__devitem(vscsi, vscsi*, Virtual SCSI controller, vscsi 4)dnl
_mcdev(vscsi, vscsi*, vscsi, {-major_vscsi_c-}, 600)dnl
__devitem(rmidi, rmidi*, Raw MIDI devices,midi)dnl
_mcdev(rmidi, rmidi*, rmidi, {-major_rmidi_c-}, 666)dnl
__devitem(diskmap, diskmap, Disk mapper, diskmap)dnl
_mkdev(diskmap, diskmap, {-M diskmap c major_diskmap_c 0 640 operator-})dnl
__devitem(pppx, pppx*, PPP Multiplexer, pppx 4)dnl
_mcdev(pppx, pppx*, pppx, {-major_pppx_c-}, 600)dnl
__devtitle(plat, Platform-specific devices)dnl
__devitem(bktr, bktr*, Video frame grabbers)dnl
_mcdev(bktr, bktr*, bktr, {-major_bktr_c-}, 644)dnl
__devitem(tuner, tuner*, Tuner devices, bktr)dnl
_mkdev(tuner, tuner*, {-M tuner$U c major_bktr_c Add(Mult($U, 2), 16) 644-}, 644)dnl
__devitem(pci, pci*, PCI bus devices)dnl
_mkdev(pci, pci*, {-M pci$U	c major_pci_c $U 600
	MKlist[${#MKlist[*]}]=";[ -h pci ] || ln -sf pci0 pci"-})dnl
__devitem(pdc, pdc, PDC device)dnl
__devitem(gpr, gpr*, GPR400 smartcard reader)dnl
_mcdev(gpr, gpr*, gpr, {-major_gpr_c-})dnl
__devitem(hotplug, hotplug, devices hot plugging)dnl
_mkdev(hotplug, hotplug, {-M hotplug c major_hotplug_c $U 400-})dnl
__devitem(gpio, gpio*, General Purpose Input/Output)dnl
_mcdev(gpio, gpio*, gpio, {-major_gpio_c-}, 600)dnl
_mkdev(local, local, {-test -s $T.local && sh $T.local-})dnl
