#!/bin/sh -
#
# THIS FILE AUTOMATICALLY GENERATED.  DO NOT EDIT.
# generated from:
#
#	OpenBSD: etc.landisk/MAKEDEV.md,v 1.23 2010/09/30 15:27:54 claudio Exp 
#	OpenBSD: MAKEDEV.common,v 1.54 2011/04/18 16:52:10 thib Exp 
#	OpenBSD: MAKEDEV.mi,v 1.80 2011/04/18 16:52:10 thib Exp 
#	OpenBSD: MAKEDEV.sub,v 1.14 2005/02/07 06:14:18 david Exp 
#
#
# Copyright (c) 2001-2004 Todd T. Fries <todd@OpenBSD.org>
#
# Permission to use, copy, modify, and distribute this software for any
# purpose with or without fee is hereby granted, provided that the above
# copyright notice and this permission notice appear in all copies.
#
# THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
# WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
# MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
# ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
# WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
# ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF
# OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
#
# Device "make" file.  Valid arguments:
#	all	makes all known devices, including local devices.
#		Tries to make the ``standard'' number of each type.
#	ramdisk	Ramdisk kernel devices
#	std	Standard devices
#	local	Configuration specific devices
# Disks:
#	ccd*	Concatenated disk devices
#	cd*	ATAPI and SCSI CD-ROM drives
#	ch*	SCSI media changers
#	raid*	RAIDframe disk devices
#	rd*	"rd" pseudo-disks
#	sd*	SCSI disks, including flopticals
#	vnd*	"file" pseudo-disk devices
#	wd*	"winchester" disk drives (ST506, IDE, ESDI, RLL, ...)
# Tapes:
#	st*	SCSI tape drives
# Terminal ports:
#	ttya	on-board serial port
# Pseudo terminals:
#	ptm	pty master device
#	pty*	Set of 62 master pseudo terminals
#	tty*	Set of 62 slave pseudo terminals
# Console ports:
#	ttyC-J*	wscons display devices
#	wscons	Minimal wscons devices
#	wskbd*	wscons keyboards
#	wsmouse*	wscons mice
#	wsmux	wscons keyboard/mouse mux devices
# USB devices:
#	ttyU*	USB serial ports
#	uall	All USB devices
#	ugen*	Generic USB devices
#	uhid*	Generic HID devices
#	ulpt*	Printer devices
#	urio*	Diamond Multimedia Rio 500
#	usb*	Bus control devices used by usbd for attach/detach
#	uscanner*	Scanners
# Special purpose devices:
#	audio*	Audio devices
#	bio	ioctl tunnel pseudo-device
#	bpf*	Berkeley Packet Filter
#	bthub*	Bluetooth Hubs
#	crypto	Hardware crypto access driver
#	diskmap	Disk mapper
#	fd	fd/* nodes
#	hotplug	devices hot plugging
#	lkm	Loadable kernel modules interface
#	music*	MIDI sequencer
#	nnpfs*	NNPFS filesystem node
#	pci*	PCI bus devices
#	pf*	Packet Filter
#	pppx*	PPP Multiplexer
#	radio*	FM tuner devices
#	*random	In-kernel random data source
#	rmidi*	Raw MIDI devices
#	systrace*	System call tracing device
#	tun*	Network tunnel driver
#	uk*	Unknown SCSI devices
#	video*	Video V4L2 devices
#	vscsi*	Virtual SCSI controller
PATH=/sbin:/usr/sbin:/bin:/usr/bin
T=$0

# set this to echo for Echo-Only debugging
[ "$eo" ] || eo=

hex()
{
	case $1 in
	[0-9]) echo -n $1;;
	10) echo -n a;;
	11) echo -n b;;
	12) echo -n c;;
	13) echo -n d;;
	14) echo -n e;;
	15) echo -n f;;
	esac
}

alph2d()
{
	local t="$1"
	local p="0123456789abcdefghijklmnopqrstuvwxyzABCDEFGHIJKLMNOPQRSTUVWXYZ"
	local sub=${p%${t}*}
	echo ${#sub}
}

h2d()
{
	local s="$1"
	local f=${s%*[0-9a-f]} n=${s#[0-9a-f]*}

	echo $(($(_h2d $f)*16+ $(_h2d $n) ))
}

_h2d()
{
	case $1 in
	[0-9]) echo -n $1;;
	a) echo -n 10;;
	b) echo -n 11;;
	c) echo -n 12;;
	d) echo -n 13;;
	e) echo -n 14;;
	f) echo -n 15;;
	esac
}

unt()
{
	# XXX pdksh can't seem to deal with locally scoped variables
	# in ${foo#$bar} expansions
	arg="$1"
	tmp="${arg#[a-zA-Z]*}"
	tmp="${tmp%*[a-zA-Z]}"
	while [ "$tmp" != "$arg" ]
	do
		arg=$tmp
		tmp="${arg#[a-zA-Z]*}"
		tmp="${tmp%*[a-zA-Z]}"
	done
	echo $arg
}

dodisk()
{
	[ "$DEBUG" ] && set -x
	n=$(($((${5}*${7:-16}))+${6})) count=0
	[ 0$7 -ne 8 ] && l="i j k l m n o p"
	for d in a b c d e f g h $l
	do
		M $1$2$d	b $3 $(($n+$count)) 640 operator
		M r$1$2$d	c $4 $(($n+$count)) 640 operator
		let count=count+1
	done
}

dodisk2()
{
	n=$(($(($5*${7:-16}))+$6))
	M $1$2a b $3 $n 640 operator
	M r$1$2a c $4 $n 640 operator
	n=$(($n+2))
	M $1$2c b $3 $n 640 operator
	M r$1$2c c $4 $n 640 operator
}

# M name b/c major minor [mode] [group]
RMlist[0]="rm -f"

mkl() {
	mklist[${#mklist[*]}]=";mknod -m $1 $2 $3 $4 $5"
}

M() {
	RMlist[${#RMlist[*]}]=$1
	mkl ${5-666} $1 $2 $3 $4
	G=${6:-wheel}
	[ "$7" ] && {
		MKlist[${#MKlist[*]}]=";chown $7:$G $1"
	} || {
		case $G in
		wheel)
			[ ${#whlist[*]} = 0 ] && whlist[0]=";chgrp wheel"
			whlist[${#whlist[*]}]="$1"
		;;
		operator)
			[ ${#oplist[*]} = 0 ] && oplist[0]=";chgrp operator"
			oplist[${#oplist[*]}]="$1"
		;;
		*)
			MKlist[${#MKlist[*]}]=";chgrp $G $1";
		esac
	}
	return 0
}

R() {
[ "$DEBUG" ] && set -x
for i in "$@"
do
U=`unt $i`
[ "$U" ] || U=0

case $i in
ramdisk)
	R std bpf0 wd0 wd1 sd0 tty00 rd0 wsmouse
	R st0 ttyC0 wskbd0 apm bio diskmap
	;;

std)
	M console	c 0 0 600
	M tty		c 1 0
	M mem		c 2 0 640 kmem
	M kmem		c 2 1 640 kmem
	M null		c 2 2
	M zero		c 2 12
	M stdin		c 7 0
	M stdout	c 7 1
	M stderr	c 7 2
	M ksyms		c 8 0 640 kmem
	M klog		c 6 0 600
	;;

vscsi*)
	M vscsi$U c 99 $U 600
	;;

video*)
	M video$U  c 77 $U
	MKlist[${#MKlist[*]}]=";[ -e video ] || ln -s video$U video"
	;;

uk*)
	M uk$U c 28 $U 640 operator
	;;

tun*)
	M tun$U c 33 $U 600
	;;

systrace)
	M systrace c 50 0 644
	;;

rmidi*)
	M rmidi$U c 57 $U 666
	;;

*random)
	n=0
	for pre in " " s u a
	do
		M ${pre}random c 40 $n 644
		n=$(($n+1))
	done
	;;

radio*)
	M radio$U     c 97 $U
	MKlist[${#MKlist[*]}]=";[ -e radio ] || ln -s radio$U radio"
	;;

pppx*)
	M pppx$U c 102 $U 600
	;;

pf*)
	M pf c 46 0 600
	;;

pci*)
	M pci$U	c 88 $U 600
	MKlist[${#MKlist[*]}]=";[ -h pci ] || ln -sf pci0 pci"
	;;

nnpfs*)
	M nnpfs$U c 51 $U 600
	;;

music*)
	M music$U     c 58 $U
	M sequencer$U c 58 $(($U+128))
	MKlist[${#MKlist[*]}]=";[ -e music ] || ln -s music$U music"
	MKlist[${#MKlist[*]}]=";[ -e sequencer ] || ln -s sequencer$U sequencer"
	;;

lkm)
	M lkm c 35 0 640 _lkm
	;;

hotplug)
	M hotplug c 37 $U 400
	;;

fd)
	RMlist[${#RMlist[*]}]=";mkdir -p fd;rm -f" n=0
	while [ $n -lt 64 ];do M fd/$n c 7 $n;n=$(($n+1));done
	MKlist[${#MKlist[*]}]=";chmod 555 fd"
	;;

diskmap)
	M diskmap c 101 0 640 operator
	;;

crypto)
	M crypto c 47 0
	;;

bthub*)
	M bthub$U c 100 $U
	;;

bpf*)
	M bpf$U c 22 $U 600
	;;

bio)
	M bio c 37 0 600
	;;

audio*)
	M sound$U	c 36 $U
	M mixer$U	c 36 $(($U+16))
	M audio$U	c 36 $(($U+128))
	M audioctl$U	c 36 $(($U+192))
	MKlist[${#MKlist[*]}]=";[ -e audio ] || ln -s audio$U audio"
	MKlist[${#MKlist[*]}]=";[ -e mixer ] || ln -s mixer$U mixer"
	MKlist[${#MKlist[*]}]=";[ -e sound ] || ln -s sound$U sound"
	MKlist[${#MKlist[*]}]=";[ -e audioctl ] || ln -s audioctl$U audioctl"
	;;

uscanner*)
	M uscanner$U c 69 $U 660
	;;

usb*)
	[ "$i" = "usb" ] && u= || u=$U
	M usb$u c 64 $U 660
	;;

urio*)
	M urio$U c 67 $U 660
	;;

ulpt*)
	M ulpt$U c 66 $U 660
	;;

uhid*)
	M uhid$U c 65 $U 660
	;;

ugen*)
	n=$(($U*16))
	for j in 0{0,1,2,3,4,5,6,7,8,9} 1{0,1,2,3,4,5}
	do
		M ugen$U.$j c 70 $(($n+10#$j)) 660
	done
	;;

uall)
	R ttyU0 ttyU1 ttyU2 ttyU3 ugen0 ugen1 ulpt0 ulpt1 uhid0 uhid1
	R uhid2 uhid3 uscanner0 urio0 usb0 usb1 usb2 usb3 usb4 usb5
	R usb6 usb7
	;;

ttyU[0-9a-zA-Z])
	U=${i#ttyU*}
	o=$(alph2d $U)
	M ttyU$U c 68 $o 660 dialer uucp
	M cuaU$U c 68 $(($o+128)) 660 dialer uucp
	;;

wsmux|wsmouse|wskbd)
	M wsmouse c 63 0 600
	M wskbd c 63 1 600
	;;

wsmouse[0-9]*)
	M wsmouse$U c 62 $U 600
	;;

wskbd[0-9]*)
	M wskbd$U c 61 $U 600
	;;

wscons)
	R wsmouse0 wsmouse1 wsmouse2 wsmouse3 wskbd0 wskbd1 wskbd2
	R wskbd3 wsmux ttyCcfg ttyC0 ttyC1 ttyC2 ttyC3 ttyC4 ttyC5
	R ttyC6 ttyC7 ttyC8 ttyC9 ttyCa ttyCb
	;;

tty[C-J]*)
	U=${i##tty[C-J]}
	case $i in
	ttyC*) n=C m=0;;
	ttyD*) n=D m=256;;
	ttyE*) n=E m=512;;
	ttyF*) n=F m=768;;
	ttyG*) n=G m=1024;;
	ttyH*) n=H m=1280;;
	ttyI*) n=I m=1536;;
	ttyJ*) n=J m=1792;;
	esac
	case $U in
	[0-9a-f]) M tty$n$U c 60 $((16#$U+$m)) 600;;
	cfg) M tty${n}cfg c 60 $((255+$m)) 600;;
	*) echo bad unit $U for $i; exit 1;;
	esac
	;;

pty*)
	if [ $U -gt 15 ]; then
		echo bad unit for pty in: $i
		continue
	fi
	set -A letters p q r s t u v w x y z P Q R S T
	set -A suffixes 0 1 2 3 4 5 6 7 8 9 a b c d e f g h i j k l m n o p q \
	    r s t u v w x y z A B C D E F G H I J K L M N O P Q R S T U V W X \
	    Y Z

	name=${letters[$U]}
	n=0
	while [ $n -lt 62 ]
	do
		nam=$name${suffixes[$n]}
		off=$(($U*62))
		M tty$nam c 4 $(($off+$n))
		M pty$nam c 5 $(($off+$n))
		n=$(($n+1))
	done
	;;

ptm)
	M ptm c 98 0 666
	;;

ttya)
	M ttya c 11 0 660 dialer uucp
	;;

st*)
	n=$(($U*16))
	for pre in " " n e en
	do
		M ${pre}st$U	b 25 $n 660 operator
		M ${pre}rst$U	c 25 $n 660 operator
		n=$(($n+1))
	done
	;;

vnd*)
	dodisk vnd $U 19 19 $U 0
	;;

rd*)
	dodisk2 rd $U 18 18 $U 0
	;;

ch*)
	M ch$U c 27 $U 660 operator
	;;

cd*)
	dodisk2 cd $U 26 26 $U 0
	;;

local)
	test -s $T.local && sh $T.local
	;;

all)
	R bthub0 bthub1 bthub2 ccd0 ccd1 ccd2 ccd3 vnd0 vnd1 vnd2
	R vnd3 sd0 sd1 sd2 sd3 sd4 sd5 sd6 sd7 sd8 sd9 cd0 cd1 rd0
	R tun0 tun1 tun2 tun3 bio bpf0 bpf1 bpf2 bpf3 bpf4 bpf5 bpf6
	R bpf7 bpf8 bpf9 pty0 diskmap vscsi0 nnpfs0 ch0 ttya hotplug
	R ptm local wscons pci0 pci1 pci2 pci3 uall rmidi0 rmidi1
	R rmidi2 rmidi3 rmidi4 rmidi5 rmidi6 rmidi7 radio0 music0
	R video0 video1 audio0 audio1 audio2 uk0 random lkm crypto pf
	R systrace wd0 wd1 wd2 wd3 raid0 raid1 raid2 raid3 std st0 st1
	R fd
	;;

wd*|sd*|raid*|ccd*)
	case $i in
	wd*) dodisk wd $U 16 16 $U 0;;
	sd*) dodisk sd $U 24 24 $U 0;;
	raid*) dodisk raid $U 71 71 $U 0;;
	ccd*) dodisk ccd $U 21 21 $U 0;;
	esac
	;;

*)
	echo $i: unknown device
	;;
esac
done
}
R "$@"
{
echo -n ${RMlist[*]}
echo -n ${mklist[*]}
echo -n ${MKlist[*]}
echo -n ${whlist[*]}
echo ${oplist[*]}
} | if [ "$eo" = "echo" ]; then
        cat
else
	sh
fi
