#	$OpenBSD: disktab,v 1.1 2005/04/01 16:02:16 deraadt Exp $
#
#	@(#)disktab	5.5 (Berkeley) 2/27/91
#
# Disk geometry and partition layout tables.
# Key:
#	ty	type of disk
#	ns	#sectors/track
#	nt	#tracks/cylinder
#	nc	#cylinders/disk
#	rm	rpm, 3600 default
#	se	sector size, 512 default
#	sf	supports bad144-style bad sector forwarding
#	so	partition offsets in sectors
#	p[a-p]	partition sizes in sectors
#	b[a-p]	partition block sizes in bytes
#	f[a-p]	partition fragment sizes in bytes
#
# All partition sizes contain space
# for bad sector tables unless the
# device drivers fail to support this.
#
# Entries may also be used for other compatible drives
# with the same geometry.

rdroot|ramdiskroot|RAM-disk root FS image:\
	:ty=simulated:se#512:nc#20:nt#2:ns#128:\
	:ta=4.2BSD:oa#0:pa#5120:fa#1024:ba#8192:\
	:ob#0:pb#0:oc#0:pc#5120:

fakecdrom|Fake image for Bootable CDROM:\
	:ty=removable:se#512:nt#1:rm#350:ns#640:nc#2048:\
	:pa#1310720:oa#0:ba#8192:fa#1024:ta=ISO9660:\
	:pc#1310720:oc#0:bc#8192:fc#1024:tc=ISO9660:
